**!**

**!**

**version 12.4**

**service timestamps debug datetime msec**

**service timestamps log datetime msec**

**no service password-encryption**

**!**

**hostname R1**

**!**

**boot-start-marker**

**boot-end-marker**

**!**

**!**

**no aaa new-model**

**memory-size iomem 5**

**ip cef**

**!**

**!**

**!**

**!**

**no ip domain lookup**

**!**

**multilink bundle-name authenticated**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**archive**

**log config**

**hidekeys**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**interface Loopback0**

**ip address 10.1.0.1 255.255.255.0**

**ip ospf network point-to-point**

**!**

**interface Loopback1**

**ip address 10.1.1.1 255.255.255.0**

**ip ospf network point-to-point**

**!**

**interface Loopback2**

**ip address 10.1.2.1 255.255.255.0**

**ip ospf network point-to-point**

**!**

**interface Loopback3**

**ip address 10.1.3.1 255.255.255.0**

**ip ospf network point-to-point**

**!**

**interface FastEthernet0/0**

**ip address 10.0.0.1 255.255.255.0**

**speed 100**

**full-duplex**

**!**

**interface FastEthernet0/1**

**no ip address**

**shutdown**

**duplex auto**

**speed auto**

**!**

**router eigrp 1**

**network 10.0.0.0**

**no auto-summary**

**!**

**ip forward-protocol nd**

**!**

**!**

**no ip http server**

**no ip http secure-server**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**control-plane**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**line con 0**

**exec-timeout 0 0**

**logging synchronous**

**line aux 0**

**line vty 0 4**

**!**

**!**

**end**